|  |  |  |  |
| --- | --- | --- | --- |
| Command | Parameter | Description | Example usage |
| start | none | Start generation of pulses by sync from oscilloscope after offset | start |
| stop | none | Stop generation of pulses | stop |
| offset | 1 - Offset value | Set time offset before starting of generation pulses | offset 4 |
| width | 1 - Pulse width value | Set duration of pulses | width 10 |